{"text_format":"2","workbook":"xlsx","n_sheets":5,"sheets":["Instructions","Solution overview","Data Center Infrastructure","Data Center Infrastructure Cont","Network Infrastructure"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":5,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Instructions","index":0,"n_rows":14,"n_cols":2,"rows_kept":14,"cut":false,"hidden":false,"merged":[[11,1,11,10],[8,1,9,6],[13,1,13,9]]}
[]
[null,"Annexure A9 IaaS Specification Response Template"]
[null,"Infrastructure as a Service Solution"]
[]
[null,"Instructions for completing Annexure A9 Response Template."]
[]
[null,"1. The reponse template contains five (4) worksheets that you are required to respond to."]
[]
[null,"2. Each worksheet requires a response and evidence must be provided as an except or a specific reference , e.g. Page 15 - Section 15.3 - paragraph 7 (The example above will ensure that informaion is easy to find by the evaluating committee)."]
[]
[]
[null,"3. All the responses are to be accompanied by evidence contained in your proposal. Bidders are obligated to give factual Information. "]
[]
[null,"4. All responses will be  recorded as such and  future implementation must match with the proposed solution. "]

{"sheet":"Solution overview","index":1,"n_rows":23,"n_cols":5,"rows_kept":23,"cut":false,"hidden":false,"merged":[[3,1,3,6],[2,1,2,6]]}
[null,"Annexure A9 IaaS Specification Response Template"]
[null,"Infrastructure as a Service Solution"]
[null,"Instructions for completing this section"]
[null,"You are required to answer by providing the technology that your organisation proposes for IaaS under column C and the OEM under column D"]
[]
[null,"Solution layer","Please indicate proposed technology","OEM","Weight"]
[null,"Core Layer",null,null,1]
[null,"Data Center Layer",null,null,1]
[null,"Access Layer",null,null,1]
[null,"Wireless Layer",null,null,1]
[null,"SDN Layer",null,null,1]
[null,"Storage Layer",null,null,1]
[null,"Compute Layer",null,null,1]
[null,"Private Cloud",null,null,1]
[null,"Public Cloud",null,null,1]
[]
[]
[]
[null,"Single OEM = 15"]
[]
[null,"2  OEM = 10"]
[null,"3 OEM= 5"]
[null,"4 or more =2 "]

{"sheet":"Data Center Infrastructure","index":2,"n_rows":20,"n_cols":6,"rows_kept":20,"cut":false,"hidden":false,"merged":[[12,1,15,1],[1,0,1,1],[7,0,9,0],[10,0,11,0],[17,0,19,0],[18,1,19,1],[12,0,15,0],[3,1,3,4]]}
["Annexure A9 IaaS Specification Response Template"]
["Data Center Infrastructure"]
[null,"Instructions for completing this section"]
[null,"You are required to provide a response for each of the requirements requested in the description. All responses must be accompanied with a comment that will contain evidence and or reference to a section in your proposal. "]
[]
[null,"Sub option","Description","Weight","Response","Comment"]
[null,"Data Center Facilities","Public cloud (data center) must be locally hosted",8]
["Infrastructure as a Service - Data Centre","Data Center Storage","Productive and non-productive loads are to be managed and provisioned from the geographical locations where the applicable server environment is hosted. A clear indication must be made on how backups are costed, including any associated network costs if these are applicable.  Due to the nature of backups and the various ways that these can be optimised, bidders are requested to indicate how their solution is optimised to save costs, and outline the architecture used to manage this.  It is prudent to indicate how the off-site storage is managed and indicate illustrative recovery times in the event that a restore is required.",1]
[null,"Data Center Security","Service providers should provide a service to protect servers and applications running on the platform free from distributed denial-of-service (DDoS) attacks (up to 500 Mbit/s of protection)",1]
[null,"Data Center Monitoring","Service Providers should provide a dashboard on cloud to monitor the utilization of infrastructers, background jobs, Utilization (lock entries, CPU, memory, Disk I/O, network and OS); track the running status of cloud services and enable administrator to configure alarm rules and notifications, and respond to them quickly.",1]
["Backup and DR","Backup","The cloud platform must provide a backup and restoration platform to customize backup policies for key data and must back up data to prevent soft disasters and hardware faults such as operational errors, software errors, and potential security breaches.\r\nBackup scope requirements: \r\n(a) VM system (Windows and Linux), File system, Database (all deployed platforms).\r\n(b) Provision of backup and restoration implementation solution.\r\n(c) Ability to restore to both live and temporary location.\r\n(d) Ability to provide periodic data recovery drill on request.",1]
[null,"DR","Productive and Non-productive loads may be split into two separate geolocations, but only if QA is designed in such a manner that it can be re-provisioned as the production environment in the event of a disaster at the primary site.  Bidders must clearly indicate how their proposal will address Disaster Recovery (DR) and redundancy by means of an architectural diagram and provide an explanation on how these two separate concepts are provided for.\r\nDR Scope Requirements\r\n• The solution must support a full production environment at all layers (OS, Application, Databases, Network, Backup, etc.) \r\n• The platform is required to provide storage level replication capability",1]
["Organization Certification","BIDDER CERTIFICATION / AFFILIATION REQUIREMENTS","The bidder must be an accredited Cloud Service Provider and must have the ISO certification system of international standardization organizations.\n\nNote: All certificates must be in writing, dated, signed and on a letterhead of the entity that issued the letter.",1]
[null,null,"The bidder must have the ISO certification system of international standardization organizations.\n\nISO 27001:2013 ---Information security management \nProvide valid certificate(s) issued in the bidder's name, containing Accreditation Details and Validity Period.\n\nNote: All certificates must be in writing, dated, signed and on a letterhead of the entity that issued the letter.\n",1]
[null,null,"The bidder must have the ISO certification system of international standardization organizations.\r\n\r\nISO 27018:2014 --- Personnel data protection \r\nProvide valid certificate(s) issued in the bidder's name, containing Accreditation Details and Validity Period.\r\n\r\nNote: All certificates must be in writing, dated, signed and on a letterhead of the entity that issued the letter.\r\n",1]
[null,null,"The bidder must have the ISO certification system of international standardization organizations.\r\n\r\nISO 22301:2012 --- Business continuity system standard\r\nProvide valid certificate(s) issued in the bidder's name, containing Accreditation Details and Validity Period.\r\n\r\nNote: All certificates must be in writing, dated, signed and on a letterhead of the entity that issued the letter.\r\n",1]
[null,"BIDDER EXPERIENCE AND CAPABILITY REQUIREMENTS","The Bidder must have previous experience in Cloud Hosting.\r\na) The bidder must provide at least 2 reference letters from a client where cloud hosting services have been supplied, maintained and supported.  The reference must not be older than thirty-six (36) months.  The reference letter must be on an official letterhead of the entity giving reference to the bidder and duly signed, dated and containing the following details:\r\nb) The customer Company name and physical address;\r\nc) Customer contact person's name, telephone number and email address;\r\nd) For a Business customer: the Company Registration Number;\r\ne) Service scope of work.",1]
["High Performance Compute","HPC Computing","High Performance Computing Capability requirements:\n1.Larger format VM: support not less than 64vCPU, 1TB memory, maximum support 255vCPU, 4TB memory\n2.GPU instance: supports 8*V100 single instance, 100GB IB interconnection\n3. FPGA instance: support\nHigh-end FPGA (Xilinx) + PCIe architecture (X16) + server local NVMe SSD + 1.2T silicon optical interconnection (direct network connection between FPGA cards)\nHigh-end FPGA (Xilinx) + PCIe architecture (X16) + server local NVMe SSD + 1.2T silicon optical interconnection (direct network connection between FPGA cards)",1]
[null,"HPC Storage","Local Storage\n1.Local data exchange for calculation process\n2.Large amount of intermediate temporary data is accessed during calculations \n3.SSD, support hard disk erasable\n4.IOPS can reach 200,000, and the computing performance is improved by more than 10%",1]
[null,null,"Remote Storage\n1.Support NAS system; two nodes form redundant NAS service\n2.Lustre parallel file system supporting IB network (recommended for IOPS> 20000 in data-intensive computing scenarios)\n3.The bottom layer adopts disk and supports encryption",1]

{"sheet":"Data Center Infrastructure Cont","index":3,"n_rows":99,"n_cols":6,"rows_kept":99,"cut":false,"hidden":false,"merged":[[46,1,48,1],[51,1,52,1],[54,1,56,1],[6,0,13,0],[73,0,98,0],[1,0,1,1],[3,1,3,5],[14,0,42,0],[43,0,72,0],[16,1,19,1],[23,1,25,1],[27,1,29,1],[30,1,33,1],[40,1,42,1],[57,1,59,1],[60,1,62,1],[69,1,72,1]]}
["Annexure A9 IaaS Specification Response Template"]
["Data Center Infrastructure Cont…"]
[null,"Instructions for completing this section"]
[null,"You are required to provide a response for each of the requirements requested in the description. All responses must be accompanied with a comment that will contain evidence and or reference to a section in your proposal. "]
[]
[null,"Requirement","Options","Weight","Response","Description"]
["Server","Components of server must provide redundancy.",null,1]
[null,"must be able to provide equipment above the CPU industry average capacity as per the response template",null,1]
[null,"Proposed solution must support  short and long-range network interfacescand no Fabric Extenders will be accepted. ",null,1]
[null,"The server must support multiple CPU slots.",null,1]
[null,"Proposed solution must be compatible with the Hybrid (private and public) cloud model",null,1]
[null,"Proposed solution must be able to support the latest Microsoft, Linux environment ",null,1]
[null,"The server must have independent management portal.",null,1]
[null,"The server must at least support RAID 0,1,5,10.",null,1]
["Normal Application Level Storage","Supplier must provide at least 4 controllers covering two engines for the storage platform. These controllers must be capable of  load balancing",null,2]
[null,"Controllers of the storage platform must support Active-Active modes and provide redundancy in the event of controller failure. (ALUA and AP architecture are not accepted.)",null,2]
[null,"Storage platform must support the ability to scale out for controllers (more than 14), without there being a service interruption or downtime on the storage platform.  ","More than 14",6]
[null,null,"Equal to 14",3]
[null,null,"Less than 14",0]
[]
[null,"The storage platform must support interconnect modules of the following protocols:\n1. PCIe\n2. Infiniband\n3. RDMA (remote direct memory access)\nThe platform must NOT support 10GbE or Fibre Channel",null,2]
[null,"Dual controllers must suppprt at least 192GB of cache memory. Additional cache by means of SSD expansion is not acceptable.",null,2]
[null,"The storage platform must be an All Flash storage system, providing SSD support for either SAS SSD or NVMe SSD.",null,2]
[null,"The storage platform must support multiple drive failures (tolerance) simultaneously (more than 2 SSDs). This protection must not incur data loss, downtime or service interruption of the platform.","More than 2 SSD failue",4]
[null,null,"Support 2 SSD failue",2]
[null,null,"Less than 2 SSD failue",0]
[null,"The storage platform must support the creation of snapshots every 3 seconds, achieving and continuous data protection.",null,2]
[null,"Drive reconstruction times must be less than 40 minutes per 1TB of data.","Less than or equal to 40 minutes",4]
[null,null,"More than 40 minutes",1]
[null,null,"larger than 1hour ",0]
[null,"A minimum of 210,000 IOPS is required by the storage paltform, with the ability to scale to higher workloads when necessary. Deduplication and compression must be enabled, with the following workloads as the benchmark:\n1. Latency of less than or equal to at least 0.1ms\n2. Read and write data blocks with sizes ranging of at least 8KB to 32KB\n3. Prefilled data occupies approximately 80% of the total usable capacity\n4. 100% of random access to be attained\n5. 70% read of all total access","More than 210K IOPS",6]
[null,null,"Equial 210K IOPS",3]
[null,null,"Less than 210K IOPS",0]
[]
[null,"Storage platform must be interoperable with other storage platforms of the same manufacturer, whether they be entry level, mid level or high level platforms. This must be achieved without the use of additional appliance(s) based solutions to meet Active-Active or replication scenarios.",null,2]
[null,"Storage platforms in both data centres must be configured in an Active-Active scenario for full data availability.",null,2]
[null,"Active-Active capabilities must be natively supported by the storage platforms, without the need for additional appliance based architectures. ",null,2]
[null,"Storage platforms must support non-disruptive upgrades of disk, disk enclosures and firmware/code of controllers. Storage upgrades and patches need to have at least a 60 day upgrade preplanning window, upgrade can be completed in 1 second.",null,2]
[null,"Storage systems must be forward compatible with new generation controllers. The controller upgrade would entail zero data migration or service interruption to the storage platform.",null,2]
[null,"Storage platforms must support 32Gb Fibre Channel connectivity through host ports.",null,2]
[null,"The expansion of disks non-disruptively and full utilization of single controllers must be supported. Maximum number of drivers per controller must be realised without restriction (More or equal to 96 disks).","More than 96 disks",4]
[null,null,"Less or equal to 96 disks but more than 48",1]
[null,null,"less than 48",0]
["Core Business Level Storage","Supplier must provide at least 4 controllers covering two engines on the storage platform. These controllers must have load balancing capabilities.",null,2]
[null,"Controllers of the storage platform must support Active-Active modes and provide redundancy in the event of controller failure. (ALUA and AP architecture are not accepted.)",null,2]
[null,"Controller load balancing is required amongst all the controllers. This would entail the performance balancing of said controllers to maximize availability and reduce potential bottlenecks in the storage platforms.",null,2]
[null,"Storage platform must support the ability to scale out for controllers(more than 14),without there being a service interruption or downtime of the storage platform.","More than 14",6]
[null,null,"Equal to 14",3]
[null,null,"Less than 14",0]
[null,"The solution must cater for remote direct memory access (RDMA) for interconnection between the storage controllers.",null,2]
[null,"Dual controllers must suppprt at least 1024GB of cache memory. Additional cache by means of SSD expansion is not acceptable.",null,2]
[null,"The storage system must be an All Flash storage platform, with only support for an all NVMe drive configuration (for both controller and disk enclousure) supported.","All provide NVMe SSD",4]
[null,null,"Not all provide NVMe SSD",0]
[null,"The storage platform must support to create a snapshot every 3 seconds, achieving continuous data protection.",null,2]
[null,"The storage platform must support the tolerance of multiple drive failures simultaneously (more than 2 SSDs). This protection must not incur data loss, downtime or service interruption of the platform.","More than 2 SSD failue",4]
[null,null,"Support 2 SSD failue",2]
[null,null,"Less than 2 SSD failue",0]
[null,"The controller architecture must support multiple controller failure across two controller engines, without service interruption or business impact. This would require a tolerance of at least 7 out of 8 controller failures.","Support tolerance of failue of 7 controllers",4]
[null,null,"Support tolerance of failue of less than 7 controllers but more than 4",4]
[null,null,"Support tolerance of failue of less than 4 controllers",2]
[null,"Drive reconstruction times must be less than 15 minutes per 1TB of data.","Less than or equal to 15 minutes",4]
[null,null,"More than 15 minutes but less than 40 minutes",2]
[null,null,"more than  40 minutes",0]
[null,"Storage platform must be able to interoperate with other storage platforms of the same manufacturer, whether they be entry level, mid level or high level platforms. This must be achieved without the use of additional appliance based solutions to meet Active-Active or replication scenarios.",null,2]
[null,"Storage platforms in both data centres need to be configured in an Active-Active scenario for full data availability.",null,2]
[null,"Active-Active capabilities need to be natively supported by the storage platforms, without the need for additional appliance based architectures. ",null,2]
[null,"Storage platforms must support non-disruptive upgrades of disk, disk enclosures and firmware/code of controllers. Storage upgrades and patches need to have at least a 60 day upgrade preplanning window, upgrade can be completed in 1 second.",null,2]
[null,"Storage systems must be forwards compatible with new generation controllers. The controller upgrade would entail zero data migration or service interruption to the storage platform.",null,2]
[null,"Storage platforms must support 32Gb Fibre Channel connectivity through host ports.",null,2]
[null,"The expansion of disks non-disruptively and full utilization of single controllers must be supported. Maximum number of drivers per controller must be realised without restriction.(more than or equals to 96 disks)","More than96 disks",4]
[null,null,"Less or equal to 96 disks but more than 48",4]
[null,null,"less than 48",1]
[]
["Private Cloud","Private Cloud providers must be able to configure cloud server licenses that can provision a fixed or unlimited number of servers.",null,2]
[null,"Private Cloud providers must provide a virtual organization management capability,whereby multiple lower level virtual organisations can be created under a tenant to match the organisational and tenant models of UNISA.",null,2]
[null,"Graphical Processing Unit passthrough must me supported, allowing GPU cards on servers to be directly connected to VMs for GPU processing, or for applications that depend on GPU computing capabilities.",null,2]
[null,"Users must be able to apply for virtual disk instances on the Cloud management platform. A virtual disk provisioning service must be provided.",null,2]
[null,"Capability for granular management of the virtual disks must be available and provided, which must include, but is not limited to:\n1. Existing disk list\n2. Disk name and status\n3. Disk capacity\n4. Attached server\n5. Disk creation time\nUsers must be able to quickly find a disk or disk group based on the name or attached status.",null,2]
[null,"Obtained virtual disks can be attached to one, or multiple, existing VMs or physical machines. This needs to be done on the Cloud management platform by users.\nUsers are also able to unattach virtual disks from one VM, and reattach to another VM or physical server.",null,2]
[null,"Private Cloud system must support the provisioning of Bare Metal Servers (BMS) as well as the integrated management of BMS environments.",null,2]
[null,"After a BMS request, the Cloud system must be able to automatically attach the data disks for the BMS without additional operational intervention on the storage management console.",null,2]
[null,"BMS must support Cloud based storage. Cloud disk can be attached to the BMS on the Cloud management platform by users, without intervention or additional operational intervention on the storage management console.",null,2]
[null,"The Cloud system must allow end users, not administrators, to create and modify backups for the Cloud service for BMS's. Users must be allowed to specify their backup policies.",null,2]
[null,"End users, and not administrators, must be allowed to manage the backup cloud service for BMS's.",null,2]
[null,"End users, and not administrators, must be allowed to restore data from BMS backups using the Cloud management platform.",null,2]
[null,"Private VM images must be able to be created by users on the Cloud management platform, this functionality must be provided.",null,2]
[null,"The sharing of the private VM images must be allowable by end users on the Cloud management platform, this functionality must be provided.",null,2]
[null,"End users must be capable of setting up the IPSec information for the VPN, this functionality must be provided.",null,2]
[null,"End users must be able to apply floating IP's and bind these IP's to Cloud or BMS servers, as well as unbinding and releasing the floating IP's.",null,2]
[null,"Cloud system operators must be able to manage and dispatch the floating IP's to any division of UNISA.",null,2]
[null,"Virtual Firewalls be provided: End users must be able to apply for virtual firewalls and be able to configure virtual firewalls through the Cloud system management platform in order to protect their assets. End users should also be able to import and export firewall rules in batches.",null,2]
[null,"Tenant level VM backup services must be enabled and provided on the Cloud platform, allowing end users, not administrators, to create and modify backups for the Cloud service for VM's. Users must be allowed to specify their backup policies.",null,2]
[null,"End users, and not administrators, must be allowed to manage the backup cloud service for VM's.",null,2]
[null,"End users, and not administrators, must be allowed to restore data from VM backups using the Cloud management platform.",null,2]
[null,"Tenant level disk backups services must be enabled and provided on the Cloud platform, allowing end users and not administrators to create the backup cloud service for specific virtual disks on the Cloud management system, allowing users to specify a backup policy.",null,2]
[null,"Backups for a specific virtual disk must be done by the end user and not the administrator. The Cloud management system must make provision for this.",null,2]
[null,"Restoration of data to specific virtual disks from virtual disk backups on the Cloud management platform must be enable for end users but not administrators. ",null,2]
[null,"Tenant level DR services must be enabled and provided on the Cloud platform, allowing the end users to create and configure a cross DC disaster recovery strategy for specific VM's and BMS environments. End users should be able to customise the DR protection policies.",null,2]
[null,"Disaster recovery testing needs to be allowed for the end users, but not the administrators. The DR testing needs to be done on the Cloud management platform.",null,2]

{"sheet":"Network Infrastructure","index":4,"n_rows":52,"n_cols":7,"rows_kept":52,"cut":false,"hidden":false,"merged":[[1,0,1,1],[3,1,3,3],[6,0,13,0],[6,1,10,1],[11,1,13,1],[14,0,19,0],[14,1,19,1],[44,0,51,0],[44,1,48,1],[49,1,51,1],[20,0,24,0],[20,1,24,1],[25,0,30,0],[25,1,30,1],[31,0,43,0],[31,1,34,1],[35,1,40,1],[41,1,43,1]]}
["Annexure A9 IaaS Specification Response Template"]
["Network Infrastructure"]
[null,"Instructions for completing this section"]
[null,"You are required to provide a response for each of the requirements requested in the description. All responses must be accompanied with a comment that will contain evidence and or reference to a section in your proposal. "]
[]
[null,"Sub option","Description","Weights","Response","Description","Scoring Criteria"]
["Data center switch","Spine","In line withr CLOS DC design guidelines, a spine and leaf topology must be followed. The spine must provide a switching capacity of 40Tbps or greater. ",4,null,null,"0: None of the 2 criteria are met;\n1: one (1) criterion met;\n2: All 2 criteria met;\n3: All 2 plus one or more additional criteria met."]
[null,null,"The DC spine must be modular with support of at least 4 line cards.",1,null,null,"0: None of the 2 criteria are met;\n1: one (1) criterion met;\n2: All 2 criteria met;\n3: All 2 plus one or more additional criteria met."]
[null,null,"DC spine layer switches must cater for 100GE support and the support of VXLAN.",1,null,null,"0: None of the 2 criteria are met;\n1: one (1) criterion met;\n2: All 2 criteria met;\n3: All 2 plus one or more additional criteria met."]
[null,null,"The DC spine layer switches must have separate management interface cards, switching forwading cards, data plane service cards and control plane service cards. ",4,null,null,"0: None of the 2 criteria are met;\n1: one (1) criterion met;\n2: All 2 criteria met;\n3: All 2 plus one or more additional criteria met."]
[null,null,"The DC spines must cater for modular cooling fans in a 1+1 redundency configuration. ",1,null,null,"0: None of the 2 criteria are met;\n1: one (1) criterion met;\n2: All 2 criteria met;\n3: All 2 plus one or more additional criteria met."]
[null,"Leaf","The switching  capacity of leaf nodes must be larger or equal to 2Tbps ",2,null,null,"0: None of the 2 criteria are met;\n1: one (1) criterion met;\n2: All 2 criteria met;\n3: All 2 plus one or more additional criteria met."]
[null,null,"Leaf node uplinks require capacity for 6 X 40GE or 6 X 100GE while downlinks must cater for 48 X 10GE. ",2,null,null,"0: None of the 2 criteria are met;\n1: one (1) criterion met;\n2: All 2 criteria met;\n3: All 2 plus one or more additional criteria met."]
[null,null,"PSU on leaf nodes should be modular with a redundent configuration of 1+1. Cooling fans need to support  a 3+1 redundent modular configuration ",1,null,null,"0: None of the 2 criteria are met;\n1: one (1) criterion met;\n2: All 2 criteria met;\n3: All 2 plus one or more additional criteria met."]
["Core LAN Switch","Core LAN ","Campus core layer switches are required to be modular and support atleast 6 service slots. ",1,null,null,"0: None of the 2 criteria are met;\n1: one (1) criterion met;\n2: All 2 criteria met;\n3: All 2 plus one or more additional criteria met."]
[null,null,"The campus core layer must support the VXLAN protocol. ",1,null,null,"0: None of the 2 criteria are met;\n1: one (1) criterion met;\n2: All 2 criteria met;\n3: All 2 plus one or more additional criteria met."]
[null,null,"The campus core layer switches should have separate management interface cards, switching forwarding cards, data plane service cards and control plane service cards. ",2,null,null,"0: None of the 2 criteria are met;\n1: one (1) criterion met;\n2: All 2 criteria met;\n3: All 2 plus one or more additional criteria met."]
[null,null,"Backplane bandwidth should equate or be greater than 10Tbps ",4,null,null,"0: None of the 2 criteria are met;\n1: one (1) criterion met;\n2: All 2 criteria met;\n3: All 2 plus one or more additional criteria met."]
[null,null,"The campus core should natively manage the wlan network to the value of 1000 access points and 10 000 users, without the need for an indepdendent WLAN service blade. ",4,null,null,"0: None of the 2 criteria are met;\n1: one (1) criterion met;\n2: All 2 criteria met;\n3: All 2 plus one or more additional criteria met."]
[null,null,"The ability to configure HQoS is a feature that is required on the campus core. ",4,null,null,"0: None of the 2 criteria are met;\n1: one (1) criterion met;\n2: All 2 criteria met;\n3: All 2 plus one or more additional criteria met."]
["Aggregation LAN Switch","Agg LAN","The campus aggregation layer needs to support a backplane bandwidth of equal or greater than 2Tbps.",4,null,null,"0: None of the 2 criteria are met;\n1: one (1) criterion met;\n2: All 2 criteria met;\n3: All 2 plus one or more additional criteria met."]
[null,null,"The aggregation layer should have the ability to natively manage the wlan network. ",4,null,null,"0: None of the 2 criteria are met;\n1: one (1) criterion met;\n2: All 2 criteria met;\n3: All 2 plus one or more additional criteria met."]
[null,null,"The campus aggregation layer would need to support the ability to manage the configuration of all switches from a master switch within the network, without the need for a controller. ",2,null,null,"0: None of the 2 criteria are met;\n1: one (1) criterion met;\n2: All 2 criteria met;\n3: All 2 plus one or more additional criteria met."]
[null,null,"Campus aggregation switch uplinks require capacity for 6 X 40GE or 6 X 100GE while downlinks should cater for 24 X 10GE. ",2,null,null,"0: None of the 2 criteria are met;\n1: one (1) criterion met;\n2: All 2 criteria met;\n3: All 2 plus one or more additional criteria met."]
[null,null,"The campus aggregation layer must be able to detect abnormal encrypted and un-encrypted traffic. ",4,null,null,"0: None of the 2 criteria are met;\n1: one (1) criterion met;\n2: All 2 criteria met;\n3: All 2 plus one or more additional criteria met."]
["Access LAN Switch","Access LAN","The campus access layer must support a backplane bandwidth of equal or greater than 200Gbps.",4,null,null,"0: None of the 2 criteria are met;\n1: one (1) criterion met;\n2: All 2 criteria met;\n3: All 2 plus one or more additional criteria met."]
[null,null,"Access layer switches require capacity of 4 X 10GE uplinks. ",4,null,null,"0: None of the 2 criteria are met;\n1: one (1) criterion met;\n2: All 2 criteria met;\n3: All 2 plus one or more additional criteria met."]
[null,null,"The access layer switches must support 3000 ipv4 or more route entries. ",4,null,null,"0: None of the 2 criteria are met;\n1: one (1) criterion met;\n2: All 2 criteria met;\n3: All 2 plus one or more additional criteria met."]
[null,null,"Uninterrupted POE must be supported by the access layer. ",4,null,null,"0: None of the 2 criteria are met;\n1: one (1) criterion met;\n2: All 2 criteria met;\n3: All 2 plus one or more additional criteria met."]
[null,null,"POE must be supported over a copper cable maximum distance of 150m or below. ",2,null,null,"0: None of the 2 criteria are met;\n1: one (1) criterion met;\n2: All 2 criteria met;\n3: All 2 plus one or more additional criteria met."]
[null,null,"Layer 3 functionality such as OSPF, ISIS and RIP should be supported. ",4,null,null,"0: None of the 2 criteria are met;\n1: one (1) criterion met;\n2: All 2 criteria met;\n3: All 2 plus one or more additional criteria met."]
["wlan","Wireless controller","The wlan controller must have the capacity to manage 4000 access points while simultaneously supporting 64 000 users. ",4,null,null,"0: None of the 2 criteria are met;\n1: one (1) criterion met;\n2: All 2 criteria met;\n3: All 2 plus one or more additional criteria met."]
[null,null,"Backplane capacity of the wlan controller must be equal to or greater than 40Gbps.",2,null,null,"0: None of the 2 criteria are met;\n1: one (1) criterion met;\n2: All 2 criteria met;\n3: All 2 plus one or more additional criteria met."]
[null,null,"The wlan controller must support 2 X 40GE and a minimum of 8 X 10GE interfaces. ",2,null,null,"0: None of the 2 criteria are met;\n1: one (1) criterion met;\n2: All 2 criteria met;\n3: All 2 plus one or more additional criteria met."]
[null,null,"The power redundency on the wlan controller should support an arrangement of 1+1.",2,null,null,"0: None of the 2 criteria are met;\n1: one (1) criterion met;\n2: All 2 criteria met;\n3: All 2 plus one or more additional criteria met."]
[null,"Indoor Access Point","Access points must support atleast 4X4 MU-MIMO mode and 802.11ax. ",4,null,null,"0: None of the 2 criteria are met;\n1: one (1) criterion met;\n2: All 2 criteria met;\n3: All 2 plus one or more additional criteria met."]
[null,null,"Max capable bandwidth must be atleast 5Gbps ",4,null,null,"0: None of the 2 criteria are met;\n1: one (1) criterion met;\n2: All 2 criteria met;\n3: All 2 plus one or more additional criteria met."]
[null,null,"Access points must support an indepdent scan feature, which can be used to shield the noise and optimize the wlan signal.",2,null,null,"0: None of the 2 criteria are met;\n1: one (1) criterion met;\n2: All 2 criteria met;\n3: All 2 plus one or more additional criteria met."]
[null,null,"Access Points must have the ability to bind two dual 5Ghz radios, providing more bandwidth to end nodes. ",4,null,null,"0: None of the 2 criteria are met;\n1: one (1) criterion met;\n2: All 2 criteria met;\n3: All 2 plus one or more additional criteria met."]
[null,null,"Access Points must have the ability to support IOT protocols. ",2,null,null,"0: None of the 2 criteria are met;\n1: one (1) criterion met;\n2: All 2 criteria met;\n3: All 2 plus one or more additional criteria met."]
[null,null,"Access Points must support atleast 2 ports (at least 1 can support 5Gbps) with the feature to logically binding these ports. ",2,null,null,"0: None of the 2 criteria are met;\n1: one (1) criterion met;\n2: All 2 criteria met;\n3: All 2 plus one or more additional criteria met."]
[null,"Outdoor Access Point","Max capable bandwidth should be atleast 5Gbps ",4,null,null,"0: None of the 2 criteria are met;\n1: one (1) criterion met;\n2: All 2 criteria met;\n3: All 2 plus one or more additional criteria met."]
[null,null,"Access points must have an IP68 rating.",2,null,null,"0: None of the 2 criteria are met;\n1: one (1) criterion met;\n2: All 2 criteria met;\n3: All 2 plus one or more additional criteria met."]
[null,null,"Access Points must support atleast 2 ports(at least 1 can support 5Gbps) with the feature to logically binding these ports. ",4,null,null,"0: None of the 2 criteria are met;\n1: one (1) criterion met;\n2: All 2 criteria met;\n3: All 2 plus one or more additional criteria met."]
["SDN","Controller & Analyzer","Must support a user to obtain the same network security access policy regardless of whether or not there is a change to the users ip address or location. ",6,null,null,"0: None of the 2 criteria are met;\n1: one (1) criterion met;\n2: All 2 criteria met;\n3: All 2 plus one or more additional criteria met."]
[null,null,"The campus SDN controller must support the automation of network configuration and  security policy configuration.",2,null,null,"0: None of the 2 criteria are met;\n1: one (1) criterion met;\n2: All 2 criteria met;\n3: All 2 plus one or more additional criteria met."]
[null,null,"The SDN solution must be able to capture and provide a view of RSSI and DBM end node WLAN variables in a historic manner. ",4,null,null,"0: None of the 2 criteria are met;\n1: one (1) criterion met;\n2: All 2 criteria met;\n3: All 2 plus one or more additional criteria met."]
[null,null,"The SDN solution must be able to proactively identify WLAN issues, provide a suggestion to resolve and AI capabilities that will allow the ability to preempt future issues.  ",4,null,null,"0: None of the 2 criteria are met;\n1: one (1) criterion met;\n2: All 2 criteria met;\n3: All 2 plus one or more additional criteria met."]
[null,null,"The SDN solution must be able to track each TCP and UDP flow on the WLAN network, providing deep packet analysis showing delay between each step in any communication stream. ",4,null,null,"0: None of the 2 criteria are met;\n1: one (1) criterion met;\n2: All 2 criteria met;\n3: All 2 plus one or more additional criteria met."]
[null,"NAC","In order to provide a better overall user experience. The network solution must have the ability to divide users on the data plane into separate IP flows using hierarchical quality of service and class of service, matching traffic based on user and application profiles.",4,null,null,"0: None of the 2 criteria are met;\n1: one (1) criterion met;\n2: All 2 criteria met;\n3: All 2 plus one or more additional criteria met."]
[null,null,"Authorization must be integrated into the network topology at the access layer edge, resulting in more secure and faster enforcement of security policies. ",4,null,null,"0: None of the 2 criteria are met;\n1: one (1) criterion met;\n2: All 2 criteria met;\n3: All 2 plus one or more additional criteria met."]
[null,null,"First time authorizations and authentications must be stored in a central database, containing unique device and network topology information. This pre-evaluated information will be used to onboard users faster during future authentications.  ",4,null,null,"0: None of the 2 criteria are met;\n1: one (1) criterion met;\n2: All 2 criteria met;\n3: All 2 plus one or more additional criteria met."]